**The single crystal diamond-based diagnostic suite of the JET tokamak for 14 MeV neutron spectroscopy measurements in DT plasmas**

D. Rigamonti1, A. Dal Molin1, G. Croci2,1, J. Figueiredo3,4, G. Gorini2,1, A. Murari1,5, A. Muraro1, M. Nocente2,1, M. Rebai1, Z. Ghani6, V. Kiptily6, E. Perelli Cippo1, M. Tardocchi1 and JET Contributors\*,

*1Institute for Plasma Science and Technology, National Research Council of Italy, Milan, Italy; 2Department of Physics, University of Milano-Bicocca, Milan, Italy;*

*3EUROfusion Programme Management Unit, Garching, Germany*

*4Instituto de Plasmas e Fusão Nuclear, Instituto Superior Técnico, Universidade de Lisboa, Lisboa, Portugal*

*5Consorzio RFX (CNR, ENEA, INFN, Università di Padova, Acciaierie Venete SpA), Corso Stati Uniti 4, 35127 Padova, Italy*

*6Culham Centre for Fusion Energy, Abingdon, United Kingdom*

Corresponding Author Email: [davide.rigamonti@istp.cnr.it](mailto:davide.rigamonti@istp.cnr.it)

In the recent year the EUROfusion enhancement program has allowed to significantly improve the JET nuclear diagnostics in view of the Deuterium-Tritium (DT) campaign. In particular, the set of the 14 MeV neutron spectrometers has been expanded with single crystal diamond-based detectors. A diamond matrix has been installed looking radially the plasma at a distance of about 20 m. In order to increase the counting statistics of the detector, it is made by 12 identical single crystal pixels working independently. Other two diamond spectrometers are single pixel diamond samples, both installed tangentially at 47 and 52 degrees with respect to the magnetic axis of the torus. The idea to using the same technology along different lines of sight allows for measuring the anisotropicity of the neutron emission which is a feature in case of use of external heating systems. Diamond detectors have been selected for their compactness, enhanced energy resolution (<1% at 14 MeV), very high count rate operation (up to 1 MHz) and high radiation hardness. They are prone to be installed on already existing fusion devices or where there are space limitations, such as on multi-lines of sight of neutron cameras.

In this paper, the suite of the diamond diagnostics will be described together with the electronics and data acquisition system, besides the detector response function to monenergetic neutrons. Typical example of measured 14 MeV neutron spectra collected during the DTE2 campaign will be also presented.

**Acknowledgments**: This work has been carried out within the framework of the EUROfusion Consortium, funded by the European Union via the Euratom Research and Training Programme (Grant Agreement No 101052200 — EUROfusion). Views and opinions expressed are however those of the author(s) only and do not necessarily reflect those of the European Union or the European Commission. Neither the European Union nor the European Commission can be held responsible for them.

\*See the author list of ‘Overview of JET results for optimising ITER operation’ by J. Mailloux et al 2022 Nucl. Fusion 62 042026